; xn77lcd.inf
; Setup information file for Mitsubishi DiamondPoint NX77LCD Monitor
;
; Copyright 2004, NEC-Mitsubishi Electronics Display, Inc.
;-------------------------------------------------
[Version]
signature="$CHICAGO$"
Class=Monitor
ClassGuid={4D36E96E-E325-11CE-BFC1-08002BE10318}
Provider=%NMD%
CatalogFile=nx77lcd.cat
DriverVer=08/31/2004,1.04.0831.2133

[ControlFlags]
ExcludeFromSelect.nt=Monitor\MEL4691
ExcludeFromSelect.nt=Monitor\MEL4692

[DestinationDirs]
NX77LCD.CopyFiles=23
DefaultDestDir=11

[SourceDisksNames]
1=%Disk1%,,,

[SourceDisksFiles]
nx77lcd.icm=1

[Manufacturer]
%NMD%=NMD

[NMD]
%NX77LCD-A%=NX77LCD-A.Install, Monitor\MEL4691
%NX77LCD-D%=NX77LCD-D.Install, Monitor\MEL4692

[NX77LCD-A.Install]
DelReg=DEL_CURRENT_REG
AddReg=NX77LCD-A.AddReg, 1280, DPMS
CopyFiles=NX77LCD.CopyFiles

[NX77LCD-D.Install]
DelReg=DEL_CURRENT_REG
AddReg=NX77LCD-D.AddReg, 1280, DPMS
CopyFiles=NX77LCD.CopyFiles

[DEL_CURRENT_REG]
HKR,MODES
HKR,,MaxResolution
HKR,,DPMS
HKR,,ICMProfile

[1280]
HKR,,MaxResolution,,"1280,1024"

[DPMS]
HKR,,DPMS,,1

[NX77LCD-A.AddReg]
HKR,"MODES\1280,1024",Mode1,,"31.0-83.0,56.0-75.0,+,+"
HKR,,ICMProfile,0,"nx77lcd.icm"

[NX77LCD-D.AddReg]
HKR,"MODES\1280,1024",Mode1,,"31.0-70.0,56.0-75.0,+,+"
HKR,,ICMProfile,0,"nx77lcd.icm"


[NX77LCD.CopyFiles]
nx77lcd.icm

[Strings]
NMD="NEC-Mitsubishi"
NX77LCD-A="Mitsubishi DiamondPoint NX77LCD (Analog)"
NX77LCD-D="Mitsubishi DiamondPoint NX77LCD (Digital)"
Disk1="NEC-Mitsubishi Monitor Installation Disk"