Пятница, 18.03.2016, 20:23
Приветствую Вас, Гость
РАДИОБЛОК
|Главная|Вход|Регистрация|

Главная » Статьи » Статьи » Библиотеки DipTrace |

3d capacitor & DipTrace

К73-17 Конденсаторы металлизированные полиэтилентерефталатные Технические условия: ТУ6261-015-07594095-2006. Защищенные изолированные конденсаторы постоянной емкости предназначены для работы в цепях постоянного, переменного и пульсирующего тока. Характеризуются высоким сопротивлением изоляции и относительно высокой температурной стабильностью параметров. Конструкция: окукленные эпоксидным компаундом, имеют одностороннее расположение выводов для печатного монтажа. Конденсаторы К73-17 предназначены для работы в цепях постоянного, переменного и пульсирующего тока. Обладают лучшеми характеристиками, чем CL21 Library DipTrace JFA - Mylar Polyester Film Capacitor Operating Temperature -40°C~ +85°C JFA - Mylar Polyester Film Capacitor Rated Voltage 100V, 250V, 400V, 630V, 1000V.DC Capacitance Range 0.001 ~ 0.47μF Capacitance Tolerance ±5%, ±10%, ±20% Insulation Resistance 0.1μF ≤30,000MΩ min, >0.1μF >15000MΩ Dissipation Factor ≤0.1 (at 1KHz) Dielectric Strength 200% of rated voltage for 5 sec. Library DipTrace WIMA Polypropylene (PP) dielectric High pulse duty Internal series connection (MKP 10 > 630 VDC, FKP 4, FKP 1) Negative capacitance change versus temperature Very low dissipation factor Self-healing properties
| A | B | C
WIMA_3A | 13 | 9 | 3
WIMA_3C | 13 | 9 | 4
WIMA_3D | 13 | 9.5 | 4
WIMA_3F | 13 | 11 | 5
WIMA_3G | 13 | 12 | 6
WIMA_3H | 13 | 12.5 | 6
WIMA_3I | 13 | 12 | 8
| A | B | C
WIMA_4B | 18 | 11 | 5
WIMA_4C | 18 | 12.5 | 6
WIMA_4D | 18 | 14 | 7
WIMA_4F | 18 | 15 | 8
WIMA_4H | 18 | 14 | 9
WIMA_4J | 18 | 16 | 9
WIMA_4M | 18 | 14 | 11
Library DipTrace EPCOS Metallized Polypropylene Film Capacitors (MKP) Features Very high pulse strength Very good self-healing properties Smallest possible dimensions High contact reliability RoHS-compatible Construction Dielectric: polypropylene (PP) Stacked-film technology Plastic case (UL 94 V-0) Epoxy resin sealing MKP_B32620 lead spacing 7.5 mm MKP_B32621 lead spacing 10 mm MKP_B32651 MKP_B32674 lead spacing 27,5 mm MKP_B32676 Capacitance value up to 270 µF High CV product, compact Good self-healing properties Over-voltage capability Low losses with high current capability High reliability Long useful life Terminals Parallel wire leads, lead-free tinned 2-pin, 4-pin and 12-pin versions Standard lead lengths: 6 1 mm lead spacing 37,5 mm MKP_B32676 lead spacing 52,5 mm Metallized Polypropylene Film Capacitors (MFP) Typical applications Smoothing Snubbering Electronic ballast Switch mode power supplies High-frequency AC loads High voltages and very high currents MFP_ B32682 lead spacing 15 mm MFP_B32683 lead spacing 22,5 mm MFP_B32684 lead spacing 27,5 mm MFP_B32686 lead spacing 37,5 mm К10-7Б_ 5мм К10-17 CL71 ------------------------------------------------------------------------------------------------------------------------------------------------------ Конденсаторы подстроечные КТ4-23 Электролитические конденсаторы 25,5х12,5мм Похожие темы: Светодиодный индикатор односимвольный Мост диодный Ремонт аккумуляторного люминесцентного светильника. продолжение следует…. При использовании материалов сайта, обязательна ссылка на сайт http://vinratel.at.ua
Категория: Библиотеки DipTrace | Добавил: RADAR62 (20.07.2014)
Просмотров: 14054 | Теги: К10-7, К73-17, К10-17, diptrace библиотеки конденсаторы, CL71, КТ4-23, JFA